Steps to install the PPC:

1)Do not install the USB dongle yet.
2)Copy all the files to the PPC machine.
3)Run Setup.exe and follow the prompts.
4)Run vcredist_86.exe and follow the instructions.
5)Reboot the PPC
6)Insert the dongle and allow windows to find the dongle automatically (see notes below if you have problems).
7)Launch the PPC and open the server view and verify the fonts have install (looks correct).
8)If fonts look wrong, then close the application and restart windows again (see notes below).
9)Install the DS_LLM by runing the Setup.exe in the DS_LLM folder.
10) Install the SeaMax Installer from the SeaLevel folder.
11)After installation, add shortcuts for PPC.EXE, DS_LLM.EXE and PiconMaker.EXE to the desktop.


Notes (Problems):

Windows 7:
If using Windows 7, you must turn off UAC (User Access Control).

Dongle Install Problems:
If you have problems installing the dongle, then use the Dongle Install.exe file in this package.
With the dongle NOT plugged in, run the Dongle Install.exe and select the top option, "USB INSTALL".
Then select "Begin Install" and wait until complete.  After completed, insert the Dongle and allow Windows to find the driver.


Font Install Problems:
If you have restarted Windows and still have font problems, then go into the
font folder under the C:\Windows directory and double click on the following fonts:
"ARIALNBI.TTF"
"ABALC.TTF"
"Absalom_.ttf"
"Alibi___.ttf"
"ARIALN.TTF"
"ARIALNB.TTF"
Restart Windows again and all should be fine.


For Windows Server 2012 R2, double click on each font and click on the "Install".

Picon Maker Problems:
Run dotNETFx35setup.exe and follow the instruction if Picon Maker is not working proper.
